(**Specifier Note**: The purpose of this guide specification is to assist the Specifier in correctly specifying styleLine fixed projection screens and their installation. The Specifier needs to edit these guide specifications to fit the needs of each specific project. References have been made within the text of the specification to MasterFormat section numbers and titles. The Specifier needs to coordinate these numbers and titles with sections included for the specific project.

Throughout the guide specification, there are Specifier Notes to assist in the editing of the file. Desired options for frame type, viewing surface, size and finish need to be noted. Brackets have been used to indicate when a selection is required. Unless noted otherwise, the first option is the standard feature. Contact a Draper, Inc. representative for further assistance with appropriate product selections. )



**SECTION 11 52 13.13**

**FIXED PROJECTION SCREENS**

Draper, Inc. StyleLine Fixed Projection Screen

1. GENERAL
	* + 1. SECTION INCLUDES
				1. Fixed projection screens.
			2. ACTION SUBMITTALS
				1. Refer to Section [**01 33 00 Submittal Procedures**] [**Insert section number and title**].
				2. Product Data: For each type of fixed projection screen, including manufacturer recommended installation procedures.
				3. Shop Drawings: Include dimensions, method of attachment and structural support.
				4. Samples: Provide finish samples.
				5. Certificate of Environmental Compliance: Documentation indicating fabrics meet or exceed the following field-validated standards set by UL GREENGUARD Environmental Institute (GEI) program for products and materials with low chemical and particle emissions for indoor usage.
			3. CLOSEOUT SUBMITTALS
				1. Refer to Section [**01 78 00 Closeout Submittals**] [**Insert section number and title**].
				2. Maintenance data.
			4. QUALITY ASSURANCE
				1. Source Limitation: Obtain fixed projection screens from single manufacturer as a complete unit including necessary mounting hardware and accessories.
			5. DELIVERY, STORAGE AND HANDLING
				1. Refer to Section [**01 60 00 Product Requirements**] [**Insert section number and title**].
				2. Deliver fixed projection screen after building is enclosed and construction within spaces where screens will be installed is substantially complete.
				3. Deliver fixed projection screens in manufacturer’s original, unopened, undamaged containers with identification labels intact.

(**Specifier Note**: Draper, Inc. does not warrant against freight damage, concealed or otherwise. RETAIN inspection and storage paragraphs below for all projects.)

* + - * 1. Inspect fixed projection screens for freight damage, concealed or otherwise, upon delivery to project site. Report damage to freight carrier immediately for replacement of fixed projection screens.
		1. Store fixed projection screens in resealed manufacturer’s original containers.
	1. WARRANTY
		1. Manufacturer limited warranty: 5 years from date of purchase.
1. PRODUCTS

(**Specifier Note**: Product information is proprietary to Draper, Inc. If additional products are required for competitive procurement, contact Draper, Inc. for assistance in listing competitive products that may be available.)

* + - 1. MANUFACTURER
				1. Draper, Inc.; 411 South Pearl Street; Spiceland, IN 47385-0425; Phone 765.987.7999; website [www.draperinc.com](http://www.draperinc.com)

Subject to compliance with requirements, manufacturers of products of equivalent design may be acceptable if approved in accordance with [**Section 01 25 00 Substitution Procedures**] [**Insert section number and title**].

* + - 1. FIXED PROJECTION SCREENS
				1. Fixed Projection Screens: Permanently tensioned projection screens fabricated by attaching viewing surface taut to perimeter frame for permanent wall installation.

Basis-of-Design: StyleLine Fixed Projection Screen.

* + - * 1. Sub Frame: Frame shall be .065 inch thick 6063 aluminum. Frame equipped with mounting flange to interface with Z-Clip wall mounting brackets. 0.5-inch (13 mm) back lip on frame to accept LED light strip (by others). Base trim frame extrusions provide for up to 1-3/8 inches (35 mm) of horizontal and vertical surface tension adjustability. Screen viewing surface is 2-3/16 inches from mounting surface.

(**Specifier Note**: StyleLine is available with two sizes of bezel or without a bezel. SELECT the frame type and mounting type below.)

Bezel Frame: [5/8-inch (16 mm)] [3-3/16 inch (81 mm)] black Vel-Tex velvety fabric-covered extruded aluminum bezel trim frame visible from the front.

Edgeless Frame: Sub frame shall be completely hidden by the projection viewing surface.

Mounting: [wall] [flown]

* + - * 1. Viewing Surface: Folded or rolled. Attaches to frame with Velcro.

(**Specifier Note**: SELECT viewing surface from one of eleven paragraphs below. Please note TecVision NanoPerf surfaces are available up to 102 inches (260 mm) image height. Contact a Draper, Inc. representative for additional assistance in selecting a viewing surface. DELETE viewing surfaces that are not project specific.)

* + 1. TecVision XH700X Premium Contrast Grey - On Axis gain of 0.7. 180 degree viewing cone. Designed for blending applications on curved or flat screens or Ultra-Short Throw (UST) projection where ambient light is present. Provides very good contrast and color reproduction. Imaging Science Foundation certified and 8K ready. Dark backing.
		2. TecVision XH1200X Premium Contrast Grey - On Axis gain of 1.2. 100 degree viewing cone. Designed to enhance contrast under controlled light. Provides excellent color reproduction. Imaging Science Foundation certified and 8K ready. Dark backing.
		3. TecVision XH800X ALR - 0.8 gain. Rejects 57% of off-axis ambient light, supports extremely wide viewing angles. Lens/Throw distance ratio for best brightness uniformity: 0.7:1 or longer. Imaging Science Foundation certified. 8K ready. Dark backing.
		4. TecVision XH900X ALR - On Axis gain of 0.9. 180 degree viewing cone. Provides very good contrast and color reproduction. Imaging Science Foundation certified and 8K ready.
		5. TecVision MS1000X ALR - On Axis gain of 1.0. 70 degree viewing cone. Provides excellent contrast and color reproduction. Performs well in ambient light. Imaging Science Foundation certified. 8K ready.
		6. TecVision CS1100X ALR - On Axis gain of 1.1. Rejects 82% of ambient light. 40 degree viewing cone. Provides excellent contrast and color reproduction. Performs well in ambient light. Imaging Science Foundation certified. 8K ready. Dark backing.
		7. TecVision XT1000X White - On Axis gain of 1.0. 180 degree viewing cone. Imaging Science Foundation certified. 8K ready reference screen surface for blending applications and Ultra-Short Throw (UST) projection. Precise resolution and color accuracy. Dark backing.
		8. TecVision XT1100X White – On Axis gain of 1.1. 180 degree viewing cone. Imaging Science Foundation certified. 8K ready reference screen surface for blending applications, precise resolution, and color accuracy.
		9. TecVision XT1300X White - On Axis gain of 1.3. 180 degree viewing cone. Imaging Science Foundation certified. 8K ready.
		10. TecVision XT1600X White - On Axis gain of 1.6. 180 degree viewing cone. Imaging Science Foundation certified. 8K ready.
		11. TecVision XH700X Grey NanoPerf - On Axis gain of 0.7. 180 degree viewing cone. Designed for blending applications on curved or flat screens or Ultra-Short Throw (UST) projection where ambient light is present. Provides very good contrast and color reproduction. Imaging Science Foundation certified and 4K ready. Dark backing.
		12. TecVision XH1200X Grey NanoPerf - On Axis gain of 1.2. 100 degree viewing cone. Designed to enhance contrast under controlled light. Provides excellent color reproduction. Imaging Science Foundation certified and 4K ready. Dark backing.
		13. TecVision XH800X ALR NanoPerf - 0.8 gain. Rejects 57% of off-axis ambient light, supports extremely wide viewing angles. Lens/Throw distance ratio for best brightness uniformity: 0.7:1 or longer. Imaging Science Foundation certified. 4K ready. Dark backing.
		14. TecVision XH900X ALR NanoPerf - On Axis gain of 0.9. 180 degree viewing cone. Provides very good contrast and color reproduction. Imaging Science Foundation certified and 4K ready.
		15. TecVision MS1000X ALR NanoPerf - On Axis gain of 1.0. 70 degree viewing cone. Provides excellent contrast and color reproduction. Performs well in ambient light. Imaging Science Foundation certified. 4K ready.
		16. TecVision CS1100X ALR NanoPerf - On Axis gain of 1.1. Rejects 82% of ambient light. 40 degree viewing cone. Provides excellent contrast and color reproduction. Performs well in ambient light. Imaging Science Foundation certified. 4K ready. Dark backing.
		17. TecVision XT1000X White NanoPerf - On Axis gain of 1.0. 180 degree viewing cone. Imaging Science Foundation certified. 8K ready reference screen surface for blending applications and Ultra-Short Throw (UST) projection. Precise resolution and color accuracy. Dark backing.
		18. TecVision XT1100X White NanoPerf – On Axis gain of 1.1. 180 degree viewing cone. Imaging Science Foundation certified. 4K ready reference screen surface for blending applications, precise resolution, and color accuracy.
		19. TecVision XT1300X White NanoPerf - On Axis gain of 1.3. 180 degree viewing cone. Imaging Science Foundation certified. 4K ready.
		20. TecVision XT1600X White NanoPerf - On Axis gain of 1.6. 180 degree viewing cone. Imaging Science Foundation certified. 4K ready.
		21. Matt White XT1000VB – On Axis gain of 1.0. 180 degree viewing cone. GREENGUARD Gold certified. Black backing.
		22. Grey XH600V – On Axis gain of 0.6. Provides excellent contrast and color reproduction. GREENGUARD Gold certified. Available with or without black backing.
		23. ClearSound NanoPerf XT1000V. On-axis gain of 1.0. Acoustically-transparent. Viewers should be at least 10 feet (305 cm) from the screen. For use in screen sizes wider than 80 inches (203 cm).

(**Specifier Note**: StyleLine is available in sizes up to 12 feet (366 cm) wide.

E. Viewing Surface Size: [**Insert custom size**].

1. HDTV Format (16:9). Black masking borders standard.

 a). 92 inch (234 cm) diagonal, 45 x 80 inches (114 x 203 cm)

 b). 100 inch (254 cm) diagonal, 49 x 87 inches (124 x 221 cm)

 c). 106 inch (269) diagonal, 52 x 92 inches (132 x 234)

 d). 110 inch (280 cm) diagonal, 54 x 96 inches (137 x 244 cm)

 e). 119 inch (302 cm) diagonal, 58 x 104 inches (147 x 264 cm)

 f). 133 inch (338 cm) diagonal, 65 inches x 116 inches (165 x 295 cm).

 g) 161 inch (409 cm) diagonal, 79 inches x 140 inches (201 x 356 cm).

2. 16:10 Format. Black masking borders standard.

 a). 94 inch (239 cm) diagonal, 50 x 80 inches (127 x 203 cm)

 b). 109 inch (277 cm) diagonal, 57-1/2 x 92 inches (146 x 234 cm)

 c). 113 inch (287 cm) diagonal, 60 x 96 inches (152 x 244 cm)

 e). 123 inch (313 cm) diagonal, 65 x 104 inches (165 x 264 cm)

 f) 137 inch (348 cm) diagonal, 72-1/2 inches x 116 inches (184 by 295 cm).

 g.) 165 inch (419 cm) diagonal, 87-1/2 inches x 140 inches (222 by 356 cm).

3. 2:35: 1 Format. Black masking borders standard.

 a). 90 inch diagonal, 35 x 83 ½ inches

 b). 116 inch diagonal 45 inches x 107 ½ inches

 c). 135 inch diagonal 52 inches x 124 inches

 d). 150 inch diagonal 58 inches x 138 ½ inches

4. 21:9 Ultrawide Format

 a). 104 ¼ inch diagonal 40 ¼ inches x 96 inches

 b). 126 inch diagonal 49 inches x 116 inches

 c). 152 inch diagonal 59 inches x 140 inches

1. EXECUTION
	* + 1. PREPARATION

 (**Specifier Note**: Fixed projection screens can be installed in recesses to achieve a flush, borderless look. COORDINATE recessed screen size and depth with wall construction. DELETE paragraph below if recessed installation is not project specific.)

* + - * 1. Coordinate screen size, mounted depth, and required edge tolerances with construction of wall recesses to house screens.
				2. Coordinate requirements for blocking and structural supports to ensure proper installation of screens.
			1. INSTALLATION
				1. Comply with screen manufacturer's written instructions and shop drawings.

(**Specifier Note**: StyleLine Fixed projection screens are shipped with viewing surface separate from frame for attachment at site. Frames are typically site assembled.)

* + - * 1. Site-assemble screen frames, stretch viewing surface over frame and attach with proprietary snapless attachment system. Exercise care to ensure viewing surface is not soiled or damaged and that surface is taut.
				2. Install fixed projection screens at locations and heights indicated on Drawings.
				3. Provide required brackets and fasteners to install screens securely to supporting substrate. Ensure that screens are level and flat.
			1. PROTECTION
				1. Protect projection screens after installation from damage during construction operations. If damage occurs, remove and replace damaged components or entire unit as required to provide units in their original, undamaged condition.

END OF SECTION